Diagram, engineering drawing

Description automatically generated

RJ45 Module Jack to be installed at each indicated location using ANSI/ITA-568 Network cabling standards

CAT6 Plenum wiring path using J-Hooks every 10 feet for all wires

CAT6 Plenum Wire to be blue in color

RJ45 Modulars to be orange in color

Patch Cables to be red in color

All wall penetrations to be sleeved and fire stopped to meet local code

RJ45 labeling=MDF/IDF-patchpanel-patchpanelport

E.G. RM23-PPA-15

MDF established in room 23/server room